after ISA installation

· Network Configuration

============== Routing

==================== Go to Default Rule Properties and go to the Action tab and set Backup Route as Upstream Proxy Server, The Setting of the Primary Route as 
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And the setting of Backup Route as 
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Then save the setting


============ Create New Routing and let it as the Default rule
· Policy Elements


============ Schedules

==================== create schedule as the specific rule time to the employees as you see
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============ Client Address Sets

=========================== Create all the groups of clients in your internal network, And put all of IP addresses in the group as the permission you want to give it.
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· Access Policy


========== Site and content Rules

=========================== Create content rule and select the schedule you created before to this rule as you see
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in the Action tab select allow if you want to give permissions to this rule



in the Applies To Tab select client address set ... and then select the group you created as you see
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=========== Protocol Rules

====================== Create rules as the groups you created before and select the specific schedule to the specific rule

· Audi-02
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